|  |  |
| --- | --- |
| PGE PM |  |
| Site name |  |
| Date Completed |  |

* 1) As-built as approved stamped drawings.
* 2) Electrical/RF disconnect mounted on pole at PGE preapproved location. **NO LOCKS are allowed on disconnect switches.**
* 3) NOC and RF placards affixed on same side of pole as disconnect switch. Must be able to be read NOC information from ground level without visual aid.
* 4) Cabinet vertical clearances: 16’ AGL StreetSide/roadside, 10’ AGL pedestrian/restricted traffic.
* 5) Disconnect switch minimum AGL height: 8’
* 6) Landscaping left “as found or better.”
* 7) Install separate ground, but bond to PGE existing ground when available.
* 8) Was disposition of replaced pole carried out as directed by the Outdoor Lighting team? e.g., was pole delivered/disposed of as outlined on the “Notice to Proceed” letter.