============================================================਍ഀ
How to build CEPC (14298) or Intel Mainstone (14244) from Sierra Wireless's drop਍ഀ
਍ഀ
The following procedures apply to all the following Platform flavours:਍ഀ
਍ഀ
Platform flavours   Env. var. name     Arg. name for buildscript਍ഀ
=================   ==============     ========================਍ഀ
Magneto PPC x86     MAGNETO_PPC        MagnetoPPC਍ഀ
Magneto SP  x86     MAGNETO_SP         MagnetoSP਍ഀ
Ozone   PPC x86     OZONEDIR           Ozone਍ഀ
Slove   SP  x86     SLOVEDIR           Slove਍ഀ
਍ഀ
IMPORTANT NOTE: To assure a clean OS system, store the MS' AKU into distinct folders, one for each platform.਍ഀ
਍ഀ
+ Copy the Microsoft drop (x86 for PPC is named PGrine, x86 for SP is named SLove) and all the sub-folders ਍ഀ
to a root drive "C" or "D" so that a distinct folder <C or D drive>:\YourChoiceOfNameForPPC or ਍ഀ
<C or D drive>:\YourChoiceOfNameForSP is created.਍ഀ
਍ഀ
+ For Intel Mainstone (14244) build, copy the original Intel's drop ("INTEL_DBPXA27X" folder) to the folder਍ഀ
"<C or D drive>:\YourChoiceOfNameForSP\platform"਍ഀ
਍ഀ
+ Copy the Sierra Wireless Carlsbad release drop to the local machine (the build image process will sign in-place਍ഀ
all the binary components, hence these files should NOT be Read-only)਍ഀ
਍ഀ
+ Launch the cmd prompt, cd to the folder "cepc_build\watcher_vob2\SW\Dlls\SwiRIL\buildscripts"਍ഀ
under Sierra Wireless's release drop ("POCKET PC 2003" or "SMARTPHONE 2003")਍ഀ
਍ഀ
+ Set the environment setting (System vaiables) so that ਍ഀ
$(MAGNETO_PPC)="<Drive>:\YourChoiceOfNameForPPC"਍ഀ
$(MAGNETO_SP)="<Drive>:\YourChoiceOfNameForSP"਍ഀ
$(OZONEDIR)="<Drive>:\YourChoiceOfNameForPPC03"਍ഀ
$(SLOVEDIR)="<Drive>:\YourChoiceOfNameForSP03"਍ഀ
਍ഀ
enter "build_cepc_img x86 c MagnetoPPC"                    for PPC winCE 5.0 (c for clean, f for fast build)਍ഀ
enter "build_cepc_img x86 c MagnetoSP"                     for SP  winCE 5.0਍ഀ
enter "build_cepc_img x86 c Ozone"                         for PPC2003਍ഀ
enter "build_cepc_img x86 c Slove"                         for SP2003 ਍ഀ
਍ഀ
+ When the build finishes successfully, start the Platform Builder and open project workspace਍ഀ
<Drive>:\YourChoiceOfName...\release\SP_x86_retail\nk.bin for CEPC or <Drive>:\YourChoiceOfName...\release\diskimage.nb0 for ਍ഀ
Intel Mainstone board.਍ഀ
਍ഀ
+ In Platform Builder select "Connectivity Options ..." under "Target" menu਍ഀ
਍ഀ
+ Choose Ethernet for download section and hit on the Select button.਍ഀ
਍ഀ
+ A dialog will be presented with a list of CEPC target devices (if it is not listed, ਍ഀ
reset the target cepc machine while this machine is also connected to the network and wait for list to appear).਍ഀ
਍ഀ
+ Select the targer cepc device from the list and hit ok button਍ഀ
਍ഀ
+ Hit Apply and Close on "Target Device Connectivity Options" tab.਍ഀ
਍ഀ
+ Select Target->Attach Device menu item to download nk.bin to cepc machine or diskimage.nb0 to Intel Mainstone board.਍ഀ
