This file contains information about the trace mask that can be used 
for the following drivers:
- Multi-Interface driver

bit position -- meaning
0 - error
1 - warnings
2 - information
3 - extendet information


8 - IOCTL handling
12 - selective suspend
13 - selective suspend busy reason 
14 - selective suspend Idle notification handling
16 - bulk/int submit/complete

