## **Note:  Please name all files that are part of your submission with your last name and the issue the project is going to be in. For example: Smith HW SO19 Article.doc or Smith HW SO19 Draft.wif**

## **Handwoven, Issue 2020**

TITLE

Author Name

Article of at least 250 words

**Resources**

Last Name, First Name. “Article.” *Handwoven*, September/October 2006, pp. 48–51.

Last Name, First name. *Book Title*. City, State of publication: Publisher, year.

## **MATERIALS**

## **Type of Project: Inkle**

**STRUCTURE**
Structure or technique name such as Warp-faced plain weave.

**EQUIPMENT**
Inkle Loom; belt shuttle; 24 four-hole weaving tablets.

**YARNS**
***Warp and Weft:*** General Yarn Name (X yd/lb; Brand), # Color Name, yardage used yd; 5/2 pearl cotton (2,100 yd/lb; UKI), #146 Periwinkle, 104 yd.

**OTHER SUPPLIES**

Anything you used to make/finish the project such as beads, safety eyes, etc.

**DIMENSIONS**

***Width:*** 1½". ***Woven Length:*** (measured under tension on the loom) 84". ***Finished size:*** (after sewing and wet-finishing) Number of items Width" x Length" with Fringe Length (if applicable)".

## ***Project Steps (Your information may differ depending on your project, but follow this format as much as possible—if you want specific instructions on how to write up a specific type of step such as pick-up let the editors know and we can provide you with examples.) If you have pick-up of other hand-manipulated techniques and need an example of formatting, please let Christina know.***

1. Wind a warp of 96 ends 110" long on your inkle loom and thread them on tablets following the draft, Figure 1.
2. Align the tablets so that the D corner of the tablets are at the front top corner as shown in Figure 2.
3. Wind a belt shuttle with Black.
4. Weave the strap using the following tablet weaving sequence repeated for 84". The 2 outer tablets on each side are the border tablet; the 20 tablets in the middle are the pattern tablets.
	* For the pattern tablets, alternate 6 backward turns (toward you) with 6 forward turns (away from you).
	* For the border tablets, turn backward until there is too much twist buildup to proceed. Then switch to turning the border tablets forward and repeat this process. This will keep the edges clean.
5. Cut the strap from the loom leaving at least 8" unwoven warp at either end for fringe. Weave in the weft tails.
6. Finish by X (sewing instructions—maybe multiple steps).
7. Wet finish by X (if applicable).

Bio: WEAVER NAME bio should be around 20 words.